# NetWare:
installing the DOS ODI driver

The Madge ODI driver for DOS is called MCBODI.COM. To install it, follow the instructions below:

1. Run the NetWare Client INSTALL program.
2. Select Other Drivers. When prompted, put the Madge CSS Release Disk into the floppy drive.
3. Type A:\DOS as the path of the driver software.
4. Select Madge 16/4 CardBus Adapter.
5. Continue through the program. When you have finished, shut down and reboot the PC.