# Installing the MDGND.OS2 driver for MS LAN Manager

To install MDGND.OS2:

1. Run the LAN Manager SETUP utility.

2. From the Network Adapter Drivers box, select Other Drivers.

3. When prompted, insert Madge release disk 2 and press [Enter].

4. Select "Madge Smart 16/4 Ringnodes (Fastmac Plus)".

5. Select the protocols you require.

6. Save your configuration.

7. Exit SETUP.

8. Shutdown, and reboot the computer. MDGND.OS2 is now installed.