# OS/2:
installing the NDIS2 driver, MCBND.OS2

If your network operating system or network application is already installed, just update the NDIS2 driver by using LAPS or MPTS.

If you have not yet installed the network operating system software or networking application you need, click on one of the following for instructions:

IBM OS/2 Warp v4.0
IBM OS/2 Warp Connect (OS/2 LAN Requester v4.0)
IBM OS/2 Warp Connect (Peer v3.0)
Adding a NetWare Client to an OS/2 Warp Connect Peer v3.0 workstation
IBM OS/2 LAN Requester v5.0

Use LAPS or MPTS to install the driver for use with most other OS/2 networking applications including:

- IBM OS/2 LAN Requester v4.0 and v3.0
- IBM TCP/IP for OS/2 v2.0
- IBM Communications Manager/2
- EICON Access for OS/2
- IBM LAN Network Manager
- IBM NetView

The NDIS2 driver also supports the following network operating systems:

Microsoft LAN Manager
Banyan Vines

| There is no OS/2 ODI driver supplied with the Madge 16/4 CardBus Adapter, but you can run an OS/2 NetWare client over the NDIS2 driver.