# Components of the Smart Software

The tables in this section describe the components of the Smart Software and show the equivalent IBM and Novell software for each.

Table 1.0 The Smart Software and equivalent IBM LSP files

Purpose | Smart Software files | Equivalent IBM LAN Support Program files
LLC interface | SMART.EXE with LLC.SMT | DXMA0MOD.SYS with DXMC0MOD.SYS
NetBIOS interface | SMART.EXE with NETB.SMT | DXMA0MOD.SYS with DXMC0MOD.SYS and DXMT0MOD.SYS
NDIS2 interface | SMART.EXE with NDIS.SMT | IBMTOK.DOS

Table 1.1 The Smart Software and eqivalent Novell files

Purpose | Smart Software files | Equivalent Novell files
IPX interface | SMART.EXE with IPX.SMT | IPX.COM
ODI interface | SMART.EXE with ODI.SMT | TOKEN.COM
TCP/IP Protocols (for NetWare IP and LAN WorkPlace for DOS) | SMART.EXE with TCP.SMT, IP.SMT, UDP.SMT, and NOVAPI.SMT | TCPIP.EXE or WGTCPIP.EXE with LSL.COM and an ODI interface.
WinSock interface | SMART.EXE with TCP.SMT, UDP.SMT, IP.SMT, NOVAPI.SMT, VNOVAPI.386, and WINSOCK.DLL | TCPIP.EXE or VTCPIP.386 with LSL.COM, an ODI interface and WINSOCK.DLL
Reverse ARP Server program | SMART.EXE with TCP.SMT, IP.SMT, UDP.SMT, NOVAPI.SMT and RARPD.SMT | TCPIP.EXE or WGTCPIP.EXE with LSL.COM, an ODI interface, and RARPD.EXE

| If you require more NetBIOS resources than Smart NetBIOS provides, use one of the methods described at the end of this chapter for providing a NetBIOS interface, or run the Madge MNETBIOS driver with Smart LLC.