# Creating a configuration script file using an installed Ringnode

| If there is more than one Ringnode installed in your computer, the script that you create can only be run Ringnode type specified in the script file.

| When you create the script Hardware Wizard will only record information about the Ringnode and Smartrom (if fitted) configuration.

To create a configuration script using a Ringnode that is already installed in your computer:

1. Type `MWIZARD SCRIPTING [ENTER]` at the DOS prompt.

2. Click on "Change Ringnode configuration". The Select script file window appears.

3. Select "Do not load script", click on "OK". The Madge Hardware Wizard window appears.

4. Click on "Custom", select the Ringnode that you want to use to create the script.

5. Configure your Ringnode settings. Save the configuration script file.