# Installing the MDGND.OS2 driver for Microsoft LAN Manager

To install MDGND.OS2:

1. Run the LAN Manager SETUP program.

2. Select Other Drivers, from the Network Adapter Drivers box. When prompted, insert the Madge release disk.

3. Select All Madge Smart 16/4 Ringnodes (MDGND.OS2).

4. Select the protocols you require, and continue through the SETUP process.

5. Save the configuration and exit from SETUP.

6. Reboot your computer.