# Novell NetWare Client for OS/2

To install the Madge ODI driver, MADGEODI.SYS, read Novell's documentation for the OS/2 NetWare Requester, then follow the steps below:

1. Use Novell's Install program to install MADGEODI.SYS. Insert the NetWare Requester disk into a floppy drive in your computer.

2. Type INSTALL [Enter] or, if the NetWare Requester is already installed on your workstation, select the NetWare Install icon from the Novell Icon View.

3. Copy the driver, MADGEODI.SYS, from the LSS CD onto a floppy disk. (MADGEODI.SYS is located under NWARE\OS2 on the LSS CD).
4. In the LAN drivers box, type MADGEODI.SYS [Enter]. When prompted, give the path of the file (A:\). Then insert the floppy disk containing the copy of MADGEODI.SYS.

5. If you are making a non-standard configuration, edit NET.CFG to add configuration details for your Ringnode. If the following line does not appear in your NET.CFG file, insert it:
   `link driver madgeodi`

   Sample NET.CFG file for NetWare workstations

       link support
       	buffers 15 4210
       link driver madgeodi
       	max frame size 4210
       	frame token-ring

6. Shut down and reboot the computer.