# Create LSS 5.0 install disks

Madge Wizard will generate install disks for a wide range of environments by copying the necessary files from the LSS CD. Select the environment you require (you can select more than one by using the control key), select the drive you want to copy the files to, and click on create.

The following LSS 5.0 install disks can be created:

- IBM LAN Server DOS Client.
- IBM LAN Server OS/2 Client or Server.
- LSS 5.0(0) Madge Wizard Disk1.
- LSS 5.0(0) Client Drivers Disk2.
- Management agents (DMI DOS and OS/2).
- Microsoft LAN Manager DOS Client (Fastmac Plus and Smart).
- Microsoft LAN Manager OS/2 Client or Server.
- Microsoft DOS Network Client and Windows for Workgroups.
- Madge Wizard.
- NDIS DOS Client (IBM LSP, Banyan Vines, other NDIS.).
- NDIS OS/2 Client (IBM LAPS, Banyan Vines, other NDIS OS/2.).
- NetWare Client-32 (DOS and Windows 95).
- NetWare DOS Client.
- NetWare OS/2 Requester.
- NetWare Server (3.11, 3.12, 4.x).
- ODI DOS Client (NetWare/IP, Personal NetWare, LAN Workplace, other ODI.).
- ODI OS/2 Client (LAN Workplace, other ODI OS/2.).
- Remote booting without Smartrom.
- Smart software (including Winsock).
- Utilities for DOS.
- Utilities for OS/2.
- Windows 95.
- Windows NT 3.5 (DEC Alpha platforms).
- Windows NT 3.5 (Intel x86 platforms).
- Windows NT 3.5 (MIPS platforms).
- Windows NT 3.5 (PowerPC platforms).