# OS/2 Warp Connect Peer v3.0 or
OS/2 LAN Requester v4.0

1. Put the OS/2 Warp Connect CD-ROM in the CD drive.
2. Put the OS/2 Warp Connect Install disk into the floppy drive, and boot the PC.
3. At the Welcome screen, press [ENTER].
4. Select Advanced installation.
5. Continue through the program until you reach the Network Support dialog box. In that dialog box, check the Yes radio button, and click OK.
6. In the Product Selection window, check the IBM Client Products option and select IBM Peer for OS/2 or IBM LAN Requester 4.0. If you need to install OS/2 NetWare Client, you must do so later. Do not attempt to install it at this point in the setup procedure.