# Sample MADGECS.CFG file

The sample file below contains configuration information for working around possible clashes between the Madge 16/4 CardBus Adapter and sound cards.

    ; A configuration for working around possible clashes with sound cards.

    EXCLUDE_IO=A20-AFF,        ; These lines delete particular I/O ranges from the
               1A20-1AFF,      ; list of available I/O ranges that MADGECS keeps.
               2A20-2AFF,
               3A20-3AFF,
               E20-EFF;

    EXCLUDE_INT=3,5            ; This line deletes interrupts 3 and 5 from MADGECS's
                               ; list of available interrupts.

    USE_INT=10                 ; This line adds interrupt 10 to MADGECS's list of
                               ; available interrupts.