# Running PNPENABL.EXE using the command line

PNPENABL.EXE automatically locates and configures the ISA Client PnP Ringnode.

For multiple Madge PnP Ringnodes, PNPENABL.EXE locates and configures them using any available I/O addresses and IRQ channels. If you specify the /IO and /INT options, then the first adapter card found by PNPENABL.EXE is assigned these values.

To run PNPENABL.EXE from the command line, type the following at the DOS prompt:

`PNPENABL <command-line options>`